# Announcement: I have to take the project down in the next few days
> Dear User,
> 
> We are writing to inform you that we have discovered two Home Assistant integration plug-ins developed by you ( https://github.com/Andre0512/hon and https://github.com/Andre0512/pyhOn ) that are in violation of our terms of service. Specifically, the plug-ins are using our services in an unauthorized manner which is causing significant economic harm to our Company.
> We take the protection of our intellectual property very seriously and demand that you immediately cease and desist all illegal activities related to the development and distribution of these plug-ins. We also request that you remove the plug-ins from all stores and code hosting platforms where they are currently available.
> Please be advised that we will take all necessary legal action to protect our interests if you fail to comply with this notice. We reserve the right to pursue all available remedies, including but not limited to monetary damages, injunctive relief, and attorney's fees.
> We strongly urge you to take immediate action to rectify this situation and avoid any further legal action. If you have any questions or concerns, please do not hesitate to contact us.
> 
> Haier Europe Security and Governance Department

# Haier hOn
[![GitHub all releases](https://img.shields.io/github/downloads/Andre0512/hon/total?color=blue&label=total%20downloads)](https://tooomm.github.io/github-release-stats/?username=Andre0512&repository=hon)
[![GitHub](https://img.shields.io/github/license/Andre0512/hon?color=red)](https://github.com/Andre0512/hon/blob/main/LICENSE)
[![Buy Me a Coffee](https://img.shields.io/badge/Buy%20Me%20a%20Coffee-donate-orange.svg)](https://www.buymeacoffee.com/andre0512)

---
Home Assistant integration for [Haier's mobile app hOn](https://hon-smarthome.com/) based on [pyhOn](https://github.com/Andre0512/pyhon).

---

[![Supported Languages](https://img.shields.io/badge/Languages-19-royalblue)](https://github.com/Andre0512/hon#supported-languages)
[![Supported Appliances](https://img.shields.io/badge/Appliances-11-forestgreen)](https://github.com/Andre0512/hon#supported-appliances)
[![Supported Models](https://img.shields.io/badge/Models-127-yellowgreen)](https://github.com/Andre0512/hon#supported-appliances)
[![Supported Entities](https://img.shields.io/badge/Entities-317-crimson)](https://github.com/Andre0512/hon#supported-appliances)  

## Supported Appliances
_Click to expand..._

<details>
<summary>Air Conditioner</summary>

### Air Conditioner Example
![Air Conditioner](assets/example_ac.png)

### Supported Air Conditioner models
Support has been confirmed for these **22 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- AD105S2SM3FA
- AD71S2SM3FA(H)
- AS07TS4HRA-M
- AS07TS5HRA
- AS09TS4HRA-M
- AS25PBAHRA
- AS25S2SF1FA
- AS25TADHRA-2
- AS25TEDHRA(M1)
- AS25THMHRA-C
- AS25XCAHRA
- AS35PBAHRA
- AS35S2SF1FA
- AS35S2SF2FA-3
- AS35TADHRA-2
- AS35TAMHRA-C
- AS35TEDHRA(M1)
- AS35XCAHRA
- AS50S2SF1FA
- AS50S2SF2FA-1
- AS50XCAHR

#### Candy
- CY-12TAIN

### Air Conditioner Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| 10° Heating | `heat-wave` | `switch` | `10degreeHeatingStatus` |
| Air Conditioner | `air-conditioner` | `climate` | `settings` |
| Echo | `account-voice` | `switch` | `echoStatus` |
| Eco Mode | `sprout` | `switch` | `ecoMode` |
| Eco Pilot | `run` | `select` | `settings.humanSensingStatus` |
| Fan Direction Horizontal | `fan` | `select` | `settings.windDirectionHorizontal` |
| Fan Direction Vertical | `fan` | `select` | `settings.windDirectionVertical` |
| Health Mode | `medication-outline` | `switch` | `healthMode` |
| Night Mode | `bed` | `switch` | `silentSleepStatus` |
| Rapid Mode | `run-fast` | `switch` | `rapidMode` |
| Screen Display | `monitor-small` | `switch` | `screenDisplayStatus` |
| Self Cleaning | `air-filter` | `switch` | `selfCleaningStatus` |
| Self Cleaning 56 | `air-filter` | `switch` | `selfCleaning56Status` |
| Silent Mode | `volume-off` | `switch` | `muteStatus` |
| Target Temperature | `thermometer` | `number` | `settings.tempSel` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Air Temperature Outdoor | `thermometer` | `sensor` | `tempAirOutdoor` |
| Ch2O Cleaning |  | `binary_sensor` | `ch2oCleaningStatus` |
| Coiler Temperature Indoor | `thermometer` | `sensor` | `tempCoilerIndoor` |
| Coiler Temperature Outside | `thermometer` | `sensor` | `tempCoilerOutdoor` |
| Defrost Temperature Outdoor | `thermometer` | `sensor` | `tempDefrostOutdoor` |
| Filter Replacement |  | `binary_sensor` | `filterChangeStatusLocal` |
| In Air Temperature Outdoor | `thermometer` | `sensor` | `tempInAirOutdoor` |
| Indoor Temperature | `thermometer` | `sensor` | `tempIndoor` |
| Machine Status | `information` | `sensor` | `machMode` |
| Outdoor Temperature | `thermometer` | `sensor` | `tempOutdoor` |
| Program |  | `select` | `startProgram.program` |
| Program | `play` | `sensor` | `programName` |
| Selected Temperature | `thermometer` | `sensor` | `tempSel` |

</details>

<details>
<summary>Air Purifier</summary>

### Air Purifier Example
![Air Purifier](assets/example_ap.png)

### Supported Air Purifier models
Support has been confirmed for these **4 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Hoover
- HHP30C011
- HHP50CA001
- HHP50CA011
- HHP70CAH011

### Air Purifier Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Aroma Time Off | `scent-off` | `number` | `settings.aromaTimeOff` |
| Aroma Time On | `scent` | `number` | `settings.aromaTimeOn` |
| Diffuser Level | `air-purifier` | `select` | `settings.aromaStatus` |
| Light status |  | `light` | `settings.lightStatus` |
| Lock Status |  | `lock` | `lockStatus` |
| Mode | `play` | `select` | `settings.machMode` |
| Pollen Level | `flower-pollen` | `number` | `settings.pollenLevel` |
| Touch Tone | `account-voice` | `switch` | `touchToneStatus` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Air Quality | `weather-dust` | `sensor` | `airQuality` |
| CO Level |  | `sensor` | `coLevel` |
| Error | `math-log` | `sensor` | `errors` |
| Humidity |  | `sensor` | `humidityIndoor` |
| Main Filter Status | `air-filter` | `sensor` | `mainFilterStatus` |
| On | `power-cycle` | `binary_sensor` | `attributes.parameters.onOffStatus` |
| PM 10 |  | `sensor` | `pm10ValueIndoor` |
| PM 2.5 |  | `sensor` | `pm2p5ValueIndoor` |
| Pre Filter Status | `air-filter` | `sensor` | `preFilterStatus` |
| Temperature |  | `sensor` | `temp` |
| Total Work Time |  | `sensor` | `totalWorkTime` |
| VOC |  | `sensor` | `vocValueIndoor` |
| Wind Speed | `fan` | `sensor` | `windSpeed` |

</details>

<details>
<summary>Dish Washer</summary>

### Dish Washer Example
![Dish Washer](assets/example_dw.png)

### Supported Dish Washer models
Support has been confirmed for these **6 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- XIB 3B2SFS-80
- XIB 6B2D3FB

#### Hoover
- HDPN 4S603PW/E
- HFB 5B2D3FW
- HFB 6B2S3FX

#### Candy
- CF 3C7L0X

### Dish Washer Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Buzzer Disabled | `volume-off` | `switch` | `buzzerDisabled` |
| Dish Washer | `dishwasher` | `switch` | `startProgram` / `stopProgram` |
#### Configs
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Add Dish | `silverware-fork-knife` | `switch` | `startProgram.addDish` |
| Delay time | `timer-plus` | `number` | `startProgram.delayTime` |
| Eco Express | `sprout` | `switch` | `startProgram.ecoExpress` |
| Extra Dry | `hair-dryer` | `switch` | `startProgram.extraDry` |
| Half Load | `fraction-one-half` | `switch` | `startProgram.halfLoad` |
| Open Door | `door-open` | `switch` | `startProgram.openDoor` |
| Program |  | `select` | `startProgram.program` |
| Remaining Time | `timer` | `select` | `startProgram.remainingTime` |
| Temperature | `thermometer` | `select` | `startProgram.temp` |
| Three in One | `numeric-3-box-outline` | `switch` | `startProgram.threeInOne` |
| Water hard | `water` | `number` | `startProgram.waterHard` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Connection |  | `binary_sensor` | `attributes.lastConnEvent.category` |
| Door |  | `binary_sensor` | `doorStatus` |
| Error | `math-log` | `sensor` | `errors` |
| Machine Status | `information` | `sensor` | `machMode` |
| Program | `play` | `sensor` | `programName` |
| Program Phase | `washing-machine` | `sensor` | `prPhase` |
| Remaining Time | `timer` | `sensor` | `remainingTimeMM` |
| Rinse Aid | `spray-bottle` | `binary_sensor` | `rinseAidStatus` |
| Salt | `shaker-outline` | `binary_sensor` | `saltStatus` |

</details>

<details>
<summary>Hood</summary>

### Supported Hood models
Support has been confirmed for these **1 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- HADG6DS46BWIFI

### Hood Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Hood | `hvac` | `switch` | `startProgram` / `stopProgram` |
| Light status |  | `light` | `settings.lightStatus` |
| Wind Speed |  | `fan` | `settings.windSpeed` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Delay time | `clock-start` | `sensor` | `delayTime` |
| Delay time status | `clock-start` | `sensor` | `delayTimeStatus` |
| Errors | `alert-circle` | `sensor` | `errors` |
| Filter Cleaning Alarm Status |  | `sensor` | `filterCleaningAlarmStatus` |
| Filter Cleaning Status |  | `sensor` | `filterCleaningStatus` |
| Last Work Time | `clock-start` | `sensor` | `lastWorkTime` |
| Light Status | `lightbulb` | `sensor` | `lightStatus` |
| Mach Mode |  | `sensor` | `machMode` |
| On / Off Status | `lightbulb` | `sensor` | `onOffStatus` |
| Quick Delay Time Status |  | `sensor` | `quickDelayTimeStatus` |
| RGB Light Color | `lightbulb` | `sensor` | `rgbLightColors` |
| RGB Light Status | `lightbulb` | `sensor` | `rgbLightStatus` |

</details>

<details>
<summary>Induction Hob</summary>

### Supported Induction Hob models
Support has been confirmed for these **3 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- HA2MTSJ68MC
- HAIDSJ63MC

#### Candy
- CIS633SCTTWIFI

### Induction Hob Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Start Program | `pot-steam` | `button` | `startProgram` |
#### Configs
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Power Management | `timelapse` | `number` | `startProgram.powerManagement` |
| Program |  | `select` | `startProgram.program` |
| Temperature | `thermometer` | `number` | `startProgram.temp` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Connection | `wifi` | `binary_sensor` | `attributes.lastConnEvent.category` |
| Error | `math-log` | `sensor` | `errors` |
| Hob Lock |  | `binary_sensor` | `hobLockStatus` |
| Hot Status |  | `binary_sensor` | `hotStatus` |
| On | `power-cycle` | `binary_sensor` | `attributes.parameters.onOffStatus` |
| Pan Status | `pot-mix` | `binary_sensor` | `panStatus` |
| Power | `lightning-bolt` | `sensor` | `power` |
| Program | `play` | `sensor` | `programName` |
| Remaining Time | `timer` | `sensor` | `remainingTimeMM` |
| Temperature | `thermometer` | `sensor` | `temp` |

</details>

<details>
<summary>Oven</summary>

### Oven Example
![Oven](assets/example_ov.png)

### Supported Oven models
Support has been confirmed for these **2 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- HWO60SM2F3XH

#### Hoover
- HSOT3161WG

### Oven Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Oven | `thermometer` | `climate` | `settings.tempSel` |
| Oven | `toaster-oven` | `switch` | `startProgram` / `stopProgram` |
#### Configs
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Delay time | `timer-plus` | `number` | `startProgram.delayTime` |
| Preheat | `thermometer-chevron-up` | `switch` | `startProgram.preheatStatus` |
| Program |  | `select` | `startProgram.program` |
| Program Duration | `timelapse` | `number` | `startProgram.prTime` |
| Target Temperature | `thermometer` | `number` | `startProgram.tempSel` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Connection | `wifi` | `binary_sensor` | `attributes.lastConnEvent.category` |
| On | `power-cycle` | `binary_sensor` | `attributes.parameters.onOffStatus` |
| Program | `play` | `sensor` | `programName` |
| Remaining Time | `timer` | `sensor` | `remainingTimeMM` |
| Start Time | `clock-start` | `sensor` | `delayTime` |
| Temperature | `thermometer` | `sensor` | `temp` |
| Temperature Selected | `thermometer` | `sensor` | `tempSel` |

</details>

<details>
<summary>Fridge</summary>

### Fridge Example
![Fridge](assets/example_ref.png)

### Supported Fridge models
Support has been confirmed for these **11 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- HDPW5620ANPD
- HBW5519ECM
- HDW5620CNPK
- HFW7720ENMB
- HFW7819EWMP
- HSW59F18EIPT
- HTW5620DNMG

#### Hoover
- HOCE7620DX

#### Candy
- CE4T620EB
- CCE4T620EWU
- CCE4T618EW

### Fridge Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Auto-Set Mode | `thermometer-auto` | `switch` | `intelligenceMode` |
| Freezer | `snowflake-thermometer` | `climate` | `settings.tempSelZ2` |
| Freezer Temperature | `thermometer` | `number` | `settings.tempSelZ2` |
| Fridge | `thermometer` | `climate` | `settings.tempSelZ1` |
| Fridge Temperature | `thermometer` | `number` | `settings.tempSelZ1` |
| MyZone | `thermometer` | `climate` | `settings.tempSelZ3` |
| MyZone Temperature | `thermometer` | `number` | `settings.tempSelZ3` |
| Program Start | `play` | `button` | `startProgram` |
| Program Stop | `stop` | `button` | `stopProgram` |
| Super Cool | `snowflake` | `switch` | `quickModeZ1` |
| Super Freeze | `snowflake-variant` | `switch` | `quickModeZ2` |
#### Configs
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Program |  | `select` | `startProgram.program` |
| Zone | `radiobox-marked` | `select` | `startProgram.zone` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Auto-Set Mode | `thermometer-auto` | `binary_sensor` | `intelligenceMode` |
| Door1 Status Freezer | `fridge-bottom` | `binary_sensor` | `doorStatusZ2` |
| Door1 Status Fridge | `fridge-top` | `binary_sensor` | `doorStatusZ1` |
| Door2 Status Freezer | `fridge-bottom` | `binary_sensor` | `door2StatusZ2` |
| Door2 Status Fridge | `fridge-top` | `binary_sensor` | `door2StatusZ1` |
| Error | `math-log` | `sensor` | `errors` |
| Holiday Mode | `palm-tree` | `binary_sensor` | `holidayMode` |
| Humidity Level | `water-outline` | `sensor` | `humidityLevel` |
| Room Humidity | `water-percent` | `sensor` | `humidityEnv` |
| Room Temperature | `home-thermometer-outline` | `sensor` | `tempEnv` |
| Super Cool | `snowflake` | `binary_sensor` | `quickModeZ1` |
| Super Freeze | `snowflake-variant` | `binary_sensor` | `quickModeZ2` |
| Temperature Freezer | `snowflake-thermometer` | `sensor` | `tempZ2` |
| Temperature Fridge | `thermometer` | `sensor` | `tempZ1` |

</details>

<details>
<summary>Tumble Dryer</summary>

### Tumble Dryer Example
![Tumble Dryer](assets/example_td.png)

### Supported Tumble Dryer models
Support has been confirmed for these **22 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- HD80-A3959
- HD90-A3TEAM5
- HD90-A2959
- HD90-A2959S
- HD90-A3959

#### Hoover
- HLE H8A2TE-S
- HLE H9A2TCE-80
- HLE C10DCE-80
- NDE H10A2TCE-80
- NDE H10RA2TCE-80
- NDE H9A2TSBEXS-S
- NDP H9A3TCBEXS-S
- NDP4 H7A2TCBEX-S
- NDPEH9A3TCBEXS-S

#### Candy
- BCTDH7A1TE
- CSOE C10DE-80
- CSOE C10TREX-47
- CSOE H10A2DE-S
- CSOE H9A2DE-S
- ROE H9A2TCE-80
- ROE H9A3TCEX-S
- ROE H10A2TCE-07

### Tumble Dryer Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Pause Tumble Dryer | `pause` | `switch` | `pauseProgram` / `resumeProgram` |
| Tumble Dryer | `tumble-dryer` | `switch` | `startProgram` / `stopProgram` |
#### Configs
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Anti-Crease | `iron` | `switch` | `startProgram.antiCreaseTime` |
| Anti-Crease | `iron` | `switch` | `startProgram.anticrease` |
| Delay time | `timer-plus` | `number` | `startProgram.delayTime` |
| Dry Time |  | `number` | `startProgram.dryTime` |
| Dry Time | `timer` | `select` | `startProgram.dryTimeMM` |
| Dry level | `hair-dryer` | `select` | `startProgram.dryLevel` |
| Program |  | `select` | `startProgram.program` |
| Sterilization | `lotion-plus` | `switch` | `startProgram.sterilizationStatus` |
| Temperature level | `thermometer` | `number` | `startProgram.tempLevel` |
| Tumbling | `refresh-circle` | `switch` | `startProgram.tumblingStatus` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Anti-Crease | `iron` | `binary_sensor` | `anticrease` |
| Connection |  | `binary_sensor` | `attributes.lastConnEvent.category` |
| Door |  | `binary_sensor` | `doorStatus` |
| Dry level | `hair-dryer` | `sensor` | `dryLevel` |
| Error | `math-log` | `sensor` | `errors` |
| Machine Status | `information` | `sensor` | `machMode` |
| Program | `play` | `sensor` | `programName` |
| Program Phase | `washing-machine` | `sensor` | `prPhase` |
| Remaining Time | `timer` | `sensor` | `remainingTimeMM` |
| Start Time | `clock-start` | `sensor` | `delayTime` |
| Temperature level | `thermometer` | `sensor` | `tempLevel` |

</details>

<details>
<summary>Wine Cellar</summary>

### Wine Cellar Example
![Wine Cellar](assets/example_wc.png)

### Supported Wine Cellar models
Support has been confirmed for these **2 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- HWS247FDU1
- HWS42GDAU1

### Wine Cellar Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Light |  | `light` | `settings.lightStatus` |
| Sabbath Mode | `palm-tree` | `switch` | `sabbathStatus` |
| Wine Cellar | `thermometer` | `climate` | `settings.tempSel` |
| Wine Cellar | `thermometer` | `climate` | `settings.tempSelZ2` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Error | `math-log` | `sensor` | `errors` |
| Humidity | `water-percent` | `sensor` | `humidityZ1` |
| Humidity 2 | `water-percent` | `sensor` | `humidityZ2` |
| Program | `play` | `sensor` | `programName` |
| Room Temperature | `home-thermometer-outline` | `sensor` | `tempEnv` |
| Selected Temperature | `thermometer` | `sensor` | `tempSel` |
| Selected Temperature 2 | `thermometer` | `sensor` | `tempSelZ2` |
| Temperature | `thermometer` | `sensor` | `temp` |
| Temperature 2 | `thermometer` | `sensor` | `tempZ2` |

</details>

<details>
<summary>Washer Dryer</summary>

### Washer Dryer Example
![Washer Dryer](assets/example_wd.png)

### Supported Washer Dryer models
Support has been confirmed for these **15 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- HWD100-B14978
- HWD100-B14979
- HWD100-B14959U1
- HWD80-B14979U1

#### Hoover
- H7D 4128MBC-S
- HD 4106AMC/1-80
- HD 485AMBB/1-S
- HD 495AMC/1-S
- HDB 5106AMC/1-80
- HDD4106AMBCR-80
- HDQ 496AMBS/1-S
- HDP 4149AMBC/1-S
- HWPS4954DAMR-11

#### Candy
- RPW41066BWMR/1-S
- RPW4966BWMR/1-S

### Washer Dryer Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Auto Dose Detergent | `cup` | `switch` | `autoDetergentStatus` |
| Auto Dose Softener | `teddy-bear` | `switch` | `autoSoftenerStatus` |
| Pause Washer Dryer | `pause` | `switch` | `pauseProgram` / `resumeProgram` |
| Washer Dryer | `washing-machine` | `switch` | `startProgram` / `stopProgram` |
| Water hard | `water` | `number` | `settings.waterHard` |
#### Configs
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Acqua Plus | `water-plus` | `switch` | `startProgram.acquaplus` |
| Anti-Crease | `iron` | `switch` | `startProgram.anticrease` |
| Anti-Crease | `iron` | `switch` | `startProgram.antiCreaseTime` |
| Auto Dose Detergent | `cup` | `switch` | `startProgram.autoDetergentStatus` |
| Auto Dose Softener | `teddy-bear` | `switch` | `startProgram.autoSoftenerStatus` |
| Delay Status | `timer-check` | `switch` | `startProgram.delayStatus` |
| Delay Time | `timer-plus` | `number` | `startProgram.delayTime` |
| Dirty level | `liquid-spot` | `select` | `startProgram.dirtyLevel` |
| Dry Time |  | `number` | `startProgram.dryTime` |
| Dry Time | `timer` | `select` | `startProgram.dryTimeMM` |
| Dry level | `hair-dryer` | `select` | `startProgram.dryLevel` |
| Extra Rinse 1 | `numeric-1-box-multiple-outline` | `switch` | `startProgram.extraRinse1` |
| Extra Rinse 2 | `numeric-2-box-multiple-outline` | `switch` | `startProgram.extraRinse2` |
| Extra Rinse 3 | `numeric-3-box-multiple-outline` | `switch` | `startProgram.extraRinse3` |
| Good Night | `weather-night` | `switch` | `startProgram.goodNight` |
| Hygiene | `lotion-plus` | `switch` | `startProgram.hygiene` |
| Keep Fresh | `refresh-circle` | `switch` | `startProgram.permanentPressStatus` |
| Main Wash Time | `clock-start` | `number` | `startProgram.mainWashTime` |
| Prewash | `tshirt-crew` | `switch` | `startProgram.prewash` |
| Program |  | `select` | `startProgram.program` |
| Rinse Iterations | `rotate-right` | `number` | `startProgram.rinseIterations` |
| Soak Prewash Selection | `tshirt-crew` | `switch` | `startProgram.haier_SoakPrewashSelection` |
| Spin speed | `numeric` | `select` | `startProgram.spinSpeed` |
| Stain Type | `liquid-spot` | `select` | `startProgram.extendedStainType` |
| Steam level | `weather-dust` | `select` | `startProgram.steamLevel` |
| Sterilization | `lotion-plus` | `switch` | `startProgram.sterilizationStatus` |
| Temperature | `thermometer` | `select` | `startProgram.temp` |
| Temperature level | `thermometer` | `number` | `startProgram.tempLevel` |
| Tumbling | `refresh-circle` | `switch` | `startProgram.tumblingStatus` |
| Water hard | `water` | `number` | `startProgram.waterHard` |
| lang |  | `number` | `startProgram.lang` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Acqua Plus | `water-plus` | `binary_sensor` | `acquaplus` |
| Anti-Crease | `iron` | `binary_sensor` | `anticrease` |
| Current Electricity Used | `lightning-bolt` | `sensor` | `currentElectricityUsed` |
| Current Temperature | `thermometer` | `sensor` | `temp` |
| Current Water Used | `water` | `sensor` | `currentWaterUsed` |
| Dirty level | `liquid-spot` | `sensor` | `dirtyLevel` |
| Door |  | `binary_sensor` | `doorStatus` |
| Door Lock |  | `binary_sensor` | `doorLockStatus` |
| Dry level | `hair-dryer` | `sensor` | `dryLevel` |
| Error | `math-log` | `sensor` | `errors` |
| Extra Rinse 1 | `numeric-1-box-multiple-outline` | `binary_sensor` | `extraRinse1` |
| Extra Rinse 2 | `numeric-2-box-multiple-outline` | `binary_sensor` | `extraRinse2` |
| Extra Rinse 3 | `numeric-3-box-multiple-outline` | `binary_sensor` | `extraRinse3` |
| Good Night Mode | `weather-night` | `binary_sensor` | `goodNight` |
| Machine Status | `information` | `sensor` | `machMode` |
| Pre Wash | `tshirt-crew` | `binary_sensor` | `prewash` |
| Program | `play` | `sensor` | `programName` |
| Program Phase | `washing-machine` | `sensor` | `prPhase` |
| Remaining Time | `timer` | `sensor` | `remainingTimeMM` |
| Remote Control | `remote` | `binary_sensor` | `attributes.lastConnEvent.category` |
| Spin Speed | `speedometer` | `sensor` | `spinSpeed` |
| Stain Type | `liquid-spot` | `sensor` | `stainType` |
| Start Time | `clock-start` | `sensor` | `delayTime` |
| Steam level | `weather-dust` | `sensor` | `steamLevel` |
| Temperature level | `thermometer` | `sensor` | `tempLevel` |
| Total Power |  | `sensor` | `totalElectricityUsed` |
| Total Wash Cycle | `counter` | `sensor` | `totalWashCycle` |
| Total Water |  | `sensor` | `totalWaterUsed` |

</details>

<details>
<summary>Washing Machine</summary>

### Washing Machine Example
![Washing Machine](assets/example_wm.png)

### Supported Washing Machine models
Support has been confirmed for these **39 models**, but many more will work. Please add already supported devices [with this form to complete the list](https://forms.gle/bTSD8qFotdZFytbf8).

#### Haier
- HW80-B14959TU1
- HW80-B14959S8U1S
- HW80-B14979TU1
- HW90-B145XLINEDE
- HW90-B14959U1
- HW90-B14959S8U1
- HW90-B14TEAM5
- HW90G-BD14979UD
- HW100-B14959U1
- HW110-14979

#### Hoover
- H5WPB447AMBC/1-S
- H7W 412MBCR-80
- H7W 610AMBC-80
- H7W4 48MBC-S
- HLWPS495TAMBE-11
- HPS484DAMB7/1-11
- HW 28AMBS/1-S
- HW 410AMBCB/1-80
- HW 411AMBCB/1-80
- HW 48AMC/1-S
- HW 49AMC/1-80
- HW 68AMC/1-80
- HW4 37AMBS/1-S
- HW4 37XMBB/1-S
- HWB 410AMC/1-80
- HWB 414AMC/1-80
- HWE 49AMBS/1-S
- HWP 48AMBCR/1-S
- HWP 610AMBC/1-S
- HWPD 69AMBC/1-S
- HWPDQ49AMBC/1-S
- HWPD 610AMBC/1-S

#### Candy
- CO4 107T1/2-07
- CBWO49TWME-S
- RO14126DWMST-S
- RO441286DWMC4-07
- RO4H7A2TEX-S
- ROW42646DWMC-07
- RP 696BWMRR/1-S

### Washing Machine Entities
#### Controls
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Auto Dose Detergent | `cup` | `switch` | `autoDetergentStatus` |
| Auto Dose Softener | `teddy-bear` | `switch` | `autoSoftenerStatus` |
| Pause Washing Machine | `pause` | `switch` | `pauseProgram` / `resumeProgram` |
| Washing Machine | `washing-machine` | `switch` | `startProgram` / `stopProgram` |
| Water hard | `water` | `number` | `settings.waterHard` |
#### Configs
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Acqua Plus | `water-plus` | `switch` | `startProgram.acquaplus` |
| Anti-Crease | `iron` | `switch` | `startProgram.anticrease` |
| Auto Dose Detergent | `cup` | `switch` | `startProgram.autoDetergentStatus` |
| Auto Dose Softener | `teddy-bear` | `switch` | `startProgram.autoSoftenerStatus` |
| Delay Status | `timer-check` | `switch` | `startProgram.delayStatus` |
| Delay Time | `timer-plus` | `number` | `startProgram.delayTime` |
| Dirty level | `liquid-spot` | `select` | `startProgram.dirtyLevel` |
| Extra Rinse 1 | `numeric-1-box-multiple-outline` | `switch` | `startProgram.extraRinse1` |
| Extra Rinse 2 | `numeric-2-box-multiple-outline` | `switch` | `startProgram.extraRinse2` |
| Extra Rinse 3 | `numeric-3-box-multiple-outline` | `switch` | `startProgram.extraRinse3` |
| Good Night | `weather-night` | `switch` | `startProgram.goodNight` |
| Hygiene | `lotion-plus` | `switch` | `startProgram.hygiene` |
| Keep Fresh | `refresh-circle` | `switch` | `startProgram.permanentPressStatus` |
| Main Wash Time | `clock-start` | `number` | `startProgram.mainWashTime` |
| Prewash | `tshirt-crew` | `switch` | `startProgram.prewash` |
| Program |  | `select` | `startProgram.program` |
| Rinse Iterations | `rotate-right` | `number` | `startProgram.rinseIterations` |
| Soak Prewash Selection | `tshirt-crew` | `switch` | `startProgram.haier_SoakPrewashSelection` |
| Spin speed | `numeric` | `select` | `startProgram.spinSpeed` |
| Stain Type | `liquid-spot` | `select` | `startProgram.extendedStainType` |
| Steam level | `weather-dust` | `select` | `startProgram.steamLevel` |
| Temperature | `thermometer` | `select` | `startProgram.temp` |
| Water hard | `water` | `number` | `startProgram.waterHard` |
| lang |  | `number` | `startProgram.lang` |
#### Sensors
| Name | Icon | Entity | Key |
| --- | --- | --- | --- |
| Acqua Plus | `water-plus` | `binary_sensor` | `acquaplus` |
| Current Electricity Used | `lightning-bolt` | `sensor` | `currentElectricityUsed` |
| Current Temperature | `thermometer` | `sensor` | `temp` |
| Current Water Used | `water` | `sensor` | `currentWaterUsed` |
| Dirty level | `liquid-spot` | `sensor` | `dirtyLevel` |
| Door |  | `binary_sensor` | `doorStatus` |
| Door Lock |  | `binary_sensor` | `doorLockStatus` |
| Error | `math-log` | `sensor` | `errors` |
| Extra Rinse 1 | `numeric-1-box-multiple-outline` | `binary_sensor` | `extraRinse1` |
| Extra Rinse 2 | `numeric-2-box-multiple-outline` | `binary_sensor` | `extraRinse2` |
| Extra Rinse 3 | `numeric-3-box-multiple-outline` | `binary_sensor` | `extraRinse3` |
| Good Night Mode | `weather-night` | `binary_sensor` | `goodNight` |
| Machine Status | `information` | `sensor` | `machMode` |
| Pre Wash | `tshirt-crew` | `binary_sensor` | `prewash` |
| Program | `play` | `sensor` | `programName` |
| Program Phase | `washing-machine` | `sensor` | `prPhase` |
| Remaining Time | `timer` | `sensor` | `remainingTimeMM` |
| Remote Control | `remote` | `binary_sensor` | `attributes.lastConnEvent.category` |
| Spin Speed | `speedometer` | `sensor` | `spinSpeed` |
| Stain Type | `liquid-spot` | `sensor` | `stainType` |
| Steam level | `weather-dust` | `sensor` | `steamLevel` |
| Total Power |  | `sensor` | `totalElectricityUsed` |
| Total Wash Cycle | `counter` | `sensor` | `totalWashCycle` |
| Total Water |  | `sensor` | `totalWaterUsed` |

</details>


## Configuration

**Method 1**: [![Open your Home Assistant instance and start setting up a new integration.](https://my.home-assistant.io/badges/config_flow_start.svg)](https://my.home-assistant.io/redirect/config_flow_start/?domain=hon)

**Method 2**: Settings > Devices & Services > Add Integration > **Haier hOn**  
_If the integration is not in the list, you need to clear the browser cache._

## Supported Languages
Translation of internal names like programs are available for all languages which are official supported by the hOn app:
* 🇨🇳 Chinese
* 🇭🇷 Croatian
* 🇨🇿 Czech
* 🇳🇱 Dutch
* 🇬🇧 English
* 🇫🇷 French
* 🇩🇪 German
* 🇬🇷 Greek
* 🇮🇱 Hebrew
* 🇮🇹 Italian
* 🇵🇱 Polish
* 🇵🇹 Portuguese
* 🇷🇴 Romanian
* 🇷🇺 Russian
* 🇷🇸 Serbian
* 🇸🇰 Slovak
* 🇸🇮 Slovenian
* 🇪🇸 Spanish
* 🇹🇷 Turkish

## Compatiblity
Haier offers different apps for different markets. Some appliances are compatible with more than one app. This integration only supports appliances that can be controlled via hOn. Please download the hOn app and check compatibilty before you open an issue.   
The apps on this (incomplete) list have been requested so far:

| App             | Main Market   | Supported                               | Alternative                                                                     |
|-----------------|---------------|-----------------------------------------|---------------------------------------------------------------------------------|
| Haier hOn       | Europe        | :heavy_check_mark:                      |                                                                                 |
| Candy simply-Fi | Europe        | :grey_question: (only newer appliances) | [ofalvai/home-assistant-candy](https://github.com/ofalvai/home-assistant-candy) |
| Hoover Wizard   | Europe        | :grey_question: (only newer appliances) |                                                                                 |
| Haier Uhome     | China         | :x:                                     | [banto6/haier](https://github.com/banto6/haier)                                 |
| Haier U+        | China         | :x:                                     |                                                                                 |
| GE SmartHQ      | North America | :x:                                     | [simbaja/ha_gehome](https://github.com/simbaja/ha_gehome)                       |   
| Haier Evo       | Russia        | :x:                                     |                                                                                 |

## Contribute
Want to help us to support more appliances? Or add more sensors? Or help with translating? Or beautify some icons or captions? 
Check out the [project on GitHub](https://github.com/Andre0512/hon), every contribution is welcome!

| Please add your appliances data to our [hon-test-data collection](https://github.com/Andre0512/hon-test-data). <br/>This helps us to develop new features and not to break compatibility in newer versions. |
|-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------|

## Useful Links
* [GitHub repository](https://github.com/Andre0512/hon)
* [pyhOn library](https://github.com/Andre0512/pyhOn)
* [Release notes](https://github.com/Andre0512/hon/releases)
* [Discussion and help](https://github.com/Andre0512/hon/discussions)
* [Issues](https://github.com/Andre0512/hon/issues)

## Support
If you find this project helpful and would like to support its development, you can buy me a coffee! ☕

[!["Buy Me A Coffee"](https://www.buymeacoffee.com/assets/img/custom_images/orange_img.png)](https://www.buymeacoffee.com/andre0512)

Don't forget to star the repository if you found it useful! ⭐
